# SRMD Coordinator v…

Desktop edge node · auto wallet · auto public link · same ARSC rules as the APK

Connecting to local coordinator…
Status
Loading…
Reachability
—
Directory
—
Directory role
—
Active phones
0
Chain height
0
Hours this epoch (approx)
0
Referral claimable
0

## Your node

Operator address
—
Public URL (phones use this)
—

Heartbeats run automatically every 20 network minutes. After each 23h settle, claim within 23 network hours — unclaimed burns.

Backup seed & advanced
Seed phrase (back this up — it controls your SRMD)

Tunnel mode needs no router ports. Public-IP mode needs firewall/router port 9334 open.

Log